*************************** START ****************************

START TIME: 202304030954

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa7670cbc
mac h: 0xe0ccdb
crc_cal: 224
crc_read: 224
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 18528 bytes (12769 compressed) at 0x00001000 in 0.4 seconds (effective 354.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 471.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 835.4 kbit/s)...

Hash of data verified.
Wrote 1408784 bytes (846812 compressed) at 0x00010000 in 12.4 seconds (effective 911.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 16 s

Download result: PASS

*************************** END ****************************



