*************************** START ****************************

START TIME: 202303271354

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

com closed
Use time: 57 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202303271356

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600200
Update flash status done!

Wrote 27040 bytes (16908 compressed) at 0x00001000 in 1.8 seconds (effective 117.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 342.5 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 621.9 kbit/s)...

Hash of data verified.
Wrote 1569040 bytes (922026 compressed) at 0x00010000 in 81.2 seconds (effective 154.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 87 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202303271358

CONNECT BAUD: 115200
serial port open error
COM:COM4
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202303271358

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202303271358

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202303271358

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202303271358

CONNECT BAUD: 115200
serial port open error
COM:COM4
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202303271359

CONNECT BAUD: 115200
serial port open error
COM:COM4
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202303271359

CONNECT BAUD: 115200
serial port open error
COM:COM4
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202303271359

CONNECT BAUD: 115200
serial port open error
COM:COM4
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202303271400

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 27040 bytes (16908 compressed) at 0x00001000 in 1.8 seconds (effective 117.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 334.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 615.2 kbit/s)...

Hash of data verified.
Wrote 1569040 bytes (922026 compressed) at 0x00010000 in 81.2 seconds (effective 154.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 87 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202303271752

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 27040 bytes (16908 compressed) at 0x00001000 in 1.8 seconds (effective 117.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 337.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 597.8 kbit/s)...

Hash of data verified.
Wrote 1445952 bytes (872864 compressed) at 0x00010000 in 76.9 seconds (effective 150.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 84 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202303281658

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

*************************** START ****************************

START TIME: 202303281659

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 27040 bytes (16908 compressed) at 0x00001000 in 0.6 seconds (effective 361.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 452.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 643.6 kbit/s)...

Hash of data verified.
Wrote 1445952 bytes (872864 compressed) at 0x00010000 in 14.2 seconds (effective 814.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 20 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202303291614

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 27040 bytes (16908 compressed) at 0x00001000 in 0.6 seconds (effective 362.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 451.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 643.4 kbit/s)...

Hash of data verified.set STOP FLG: Truecom closed
Use time: 7 s

Download result: PASS

*************************** END ****************************



set state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202303291615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202303291615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202303291615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202303291615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
*************************** START ****************************

START TIME: 202303291615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!
*************************** START ****************************

START TIME: 202303291615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe6295acc
mac h: 0xd3e0e2
crc_cal: 211
crc_read: 211
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 27040 bytes (16908 compressed) at 0x00001000 in 0.6 seconds (effective 358.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.1 seconds (effective 437.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 593.6 kbit/s)...

Hash of data verified.
Wrote 1446096 bytes (872903 compressed) at 0x00010000 in 14.4 seconds (effective 804.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 23 s

Download result: PASS

*************************** END ****************************



