*************************** START ****************************

START TIME: 202303271524

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe99e7a4
mac h: 0xdf3ce9
crc_cal: 223
crc_read: 223
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018

*************************** START ****************************

START TIME: 202303271524

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xe99e7a4
mac h: 0xdf3ce9
crc_cal: 223
crc_read: 223
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 27040 bytes (16908 compressed) at 0x00001000 in 1.7 seconds (effective 130.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (173 compressed) at 0x00008000 in 0.0 seconds (effective 614.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.1 seconds (effective 1292.0 kbit/s)...

Hash of data verified.
Wrote 1445952 bytes (872864 compressed) at 0x00010000 in 76.6 seconds (effective 151.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 81 s

Download result: PASS

*************************** END ****************************



